### Block: Sequencer

Inports
Start | Start signal. Rising flank triggers sequence

Outports
Out1 | Output #1
Out2 | Output #2
Out3 | Output #3
Out4 | Output #4

Mask Parameters
Name | ID | Description
Delay1 | 1 | Time delay for output 1
Delay2 | 2 | Time delay for output 2
Delay3 | 3 | Time delay for output 3
Delay4 | 4 | Time delay for output 4
ts_fact | 5 | Multiplication factor of base sampling time (in integer format)

##### Description:

Generation of time delayed (enable) sequence.

##### Implementations:

Bool | Boolean Implementation
FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: Bool

Boolean Implementation

Inports Data Type
Start | bool

Outports Data Type
Out1 | bool
Out2 | bool
Out3 | bool
Out4 | bool

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
Start | int8

Outports Data Type
Out1 | int8
Out2 | int8
Out3 | int8
Out4 | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
Start | int16

Outports Data Type
Out1 | int16
Out2 | int16
Out3 | int16
Out4 | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
Start | int32

Outports Data Type
Out1 | int32
Out2 | int32
Out3 | int32
Out4 | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
Start | float32

Outports Data Type
Out1 | float32
Out2 | float32
Out3 | float32
Out4 | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
Start | float64

Outports Data Type
Out1 | float64
Out2 | float64
Out3 | float64
Out4 | float64