### Block: Limitation

Inports
In | Input signal
max | Upper limit
min | Lower limit

Outports
Out | Limited input signal

##### Description:

Limits the input signal to min and max_sci.

Caution: For correct computation the upper limit max has to be greater than the lower limit min!

Calculation:

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16
max | int16
min | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32
max | int32
min | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32
max | float32
min | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64
max | float64
min | float64

Outports Data Type
Out | float64