### Block: Selector

Inports
In0 | Input #0
In1 | Input #1
In2 | Input #2
In3 | Input #3
In4 | Input #4
In5 | Input #5
In6 | Input #6
In7 | Input #7
Select | Input select

Outports
Out | Selected input signal

##### Description:

Passing through of input signal selected by the select inport:

Select = 0 (DSP): Out = In0

Select = 1 (DSP): Out = In1

...

Select = 7 (DSP): Out = In7

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In0 | int8
In1 | int8
In2 | int8
In3 | int8
In4 | int8
In5 | int8
In6 | int8
In7 | int8
Select | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In0 | int16
In1 | int16
In2 | int16
In3 | int16
In4 | int16
In5 | int16
In6 | int16
In7 | int16
Select | int8

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In0 | int32
In1 | int32
In2 | int32
In3 | int32
In4 | int32
In5 | int32
In6 | int32
In7 | int32
Select | int8

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In0 | float32
In1 | float32
In2 | float32
In3 | float32
In4 | float32
In5 | float32
In6 | float32
In7 | float32
Select | int8

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In0 | float64
In1 | float64
In2 | float64
In3 | float64
In4 | float64
In5 | float64
In6 | float64
In7 | float64
Select | int8

Outports Data Type
Out | float64