\XtoCBlock{Inport}
\label{block:Inport}
\begin{figure}[H]\includegraphics{Inport}\end{figure} 

\begin{XtoCtabular}{Inports}
IN & Signal from frame program\\
\hline
\end{XtoCtabular}


\begin{XtoCtabular}{Mask Parameters}
ts\_fact & Multiplication factor of base sampling time (in integer format)\\
\hline
Gain & Gain value used in simulation\\
\hline
Offset & Offset value used in simulation\\
\hline
\end{XtoCtabular}

\subsubsection*{Description:}
Serves as interface to the frame program. The input of this block is intended for simulation purposes and can be left unconnected if not used. Also the parameters \textit{Gain} and \textit{Offset} are only used during simulation. The schematic for simulation can be seen in the figure below.

\textbf{Note:} Currently, \textit{Gain} and \textit{Offset} parameters are only available in Matlab/Simulink.
\begin{figure}[H]
  \includegraphics{Inport_Schematic}
\end{figure} 

\subsubsection*{Data Types:}
\begin{tblr}{l l}
\textbf{bool} & Boolean\\
\textbf{int8} & 8 Bit Fixed Point\\
\textbf{int16} & 16 Bit Fixed Point\\
\textbf{int32} & 32 Bit Fixed Point\\
\textbf{float32} & 32 Bit Floating Point\\
\textbf{float64} & 64 Bit Floating Point\\
\end{tblr}
