### Block: Biquad

Inports
In | Input In(k)

Outports
Out | Output Out(k)

Mask Parameters
Name | ID | Description
b0 | 1 | Filter coefficient b0
b1 | 2 | Filter coefficient b1
b2 | 3 | Filter coefficient b2
a0 | 4 | Filter coefficient a0
a1 | 5 | Filter coefficient a1
a2 | 6 | Filter coefficient a2
ts_fact | 7 | Multiplication factor of base sampling time (in integer format)

##### Description:

Second order transfer function:

H(z) = (b0.z2 + b1.z + b2) / (a0.z2 + a1.z + a2)

Alternative representation of the same transfer function:

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64