### Block: ACDC

Inports
In | Input signal
phi | Angle signal

Outports
AC | AC part of input signal
DC | DC part of input signal

Mask Parameters
Name | ID | Description
ts_fact | 1 | Multiplication factor of base sampling time (in integer format)

##### Description:

Calculation of AC and DC part of input signal.

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16
phi | int16

Outports Data Type
AC | int16
DC | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32
phi | int32

Outports Data Type
AC | int32
DC | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32
phi | float32

Outports Data Type
AC | float32
DC | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64
phi | float64

Outports Data Type
AC | float64
DC | float64