### Block: Outport

Outports
OUT | Signal to frame program

Mask Parameters
ts_fact | Multiplication factor of base sampling time (in integer format)
Gain | Gain value used in simulation
Offset | Offset value used in simulation

##### Description:

Serves as interface to the frame program. The output of this block is intended for simulation purposes and can be left unconnected if not used. Also the parameters Gain, and Offset are only used during simulation. The schematic for simulation can be seen in the figure below. The Unit Delay block is only used during simulation and should reflect the time delay caused by a discrete controller.

Note: Currently, Gain and Offset parameters are only available in Matlab/Simulink.

##### Data Types:

int8 | 8 Bit Fixed Point
int16 | 16 Bit Fixed Point
int32 | 32 Bit Fixed Point
float32 | 32 Bit Floating Point
float64 | 64 Bit Floating Point