### Block: SinGen

Inports
A | Amplitude
f | Frequency

Outports
u | Sine wave output

Mask Parameters
fmax | Maximum Frequency in Hz
Offset | Offset
Phase | Phase [-Pi..Pi]
ts_fact | Multiplication factor of base sampling time (in integer format)

##### Description:

Generation of a sine wave with amplitude (A) and frequency (f).

Calculation fixed point implementation:

uk = Ak sin + Aoffset |  |

For sine calculation a lookup table with 256 entries is used. This results in a short computation time but with the downside of reduced accuracy for the FiP32 implementation.

Calculation floating point implementation (parameter f_max is ignored):

uk = Ak sin + Aoffset |  |

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
A | int16
f | int16

Outports Data Type
u | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
A | int32
f | int32

Outports Data Type
u | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
A | float32
f | float32

Outports Data Type
u | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
A | float64
f | float64

Outports Data Type
u | float64