### Block: LookupTable

Inports
In | Table index

Outports
Out | Table output

Mask Parameters
Lookup | Look-up Table

##### Description:

Look-up Table with 256+1 values.

Note: 257th value is used for preventing index overflow during interpolation.

-> for periodic signals the 257th value should be set equal to 1st value

-> for non-periodic signals the 257th value should be set equal to 256th value

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32