### Block: uSaveSignal

Inports
In | Input signal to be saved

##### Description:

Makes the incoming signal accessible for reading with parameter numbers.

##### Implementations:

Bool | Boolean Implementation
FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: Bool

Boolean Implementation

Inports Data Type
In | bool

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64