### Block: DT1

Inports
In | Input In(k)

Outports
Out | Output Out(k)

Mask Parameters
Name | ID | Description
V | 1 | Gain
fc | 2 | Cut off frequency of low pass filter
ts_fact | 3 | Multiplication factor of base sampling time (in integer format)
method | 4 | Discretization method

##### Description:

First order high pass:

G(s) = V*s/(s/w + 1)

Due to limited value range in the 8 bit fixed point implementation rather high deviations from expected output values may occur.

Developer note: The source code of block TF1 is used.

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64