### Block: MinMaxPeriodic

Inports
In | Input signal
phi | Angle signal

Outports
max | Maximum of input signal
min | Minimum of input signal

##### Description:

Outputs the minimum and maximum of the input signal over one period of the (angle) signal phi.

Exemplary signal waveforms:

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16
phi | int16

Outports Data Type
max | int16
min | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32
phi | int32

Outports Data Type
max | int32
min | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32
phi | float32

Outports Data Type
max | float32
min | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64
phi | float64

Outports Data Type
max | float64
min | float64