### Block: IIR

Inports
In | Input In(k)

Outports
Out | Output Out(k)

Mask Parameters
Name | ID | Description
CoeffB | 1 | Array with filter coefficients of numerator
CoeffA | 2 | Array with filter coefficients of denominator
ts_fact | 3 | Multiplication factor of base sampling time (in integer format)

##### Description:

Transfer function:

H(z) = (b0.z^n + b1.z + ...+ bn) / (a0.z^n + a1.z + ... + an)

The maximum filter order is 32.

The order of the denominator has to be greater than or equal to the order of the numerator.

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64