### Block: Delay

Inports
In | Input In(k)

Outports
Out | Output Out(k)=In(k-1)

Mask Parameters
Name | ID | Description
ts_fact | 1 | Multiplication factor of base sampling time (in integer format)

##### Description:

Output delay by one sample time interval.

##### Implementations:

Bool | Boolean Integration
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: Bool

Boolean Integration

Inports Data Type
In | bool

Outports Data Type
Out | bool

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64