### Block: Sum

Inports
In1 | Input #1
In2 | Input #2
In3 | Input #3
In4 | Input #4
In5 | Input #5
In6 | Input #6
In7 | Input #7
In8 | Input #8

Outports
Out | Result

Mask Parameters
Name | ID | Description
In1 | 1 | Input #1
In2 | 2 | Input #2
In3 | 3 | Input #3
In4 | 4 | Input #4
In5 | 5 | Input #5
In6 | 6 | Input #6
In7 | 7 | Input #7
In8 | 8 | Input #8

##### Description:

Sum of inputs:

+ ... Input will be added to result.

- ... Input will be subtracted from result.

0 ... Input will be ignored.

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In1 | int8
In2 | int8
In3 | int8
In4 | int8
In5 | int8
In6 | int8
In7 | int8
In8 | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In1 | int16
In2 | int16
In3 | int16
In4 | int16
In5 | int16
In6 | int16
In7 | int16
In8 | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In1 | int32
In2 | int32
In3 | int32
In4 | int32
In5 | int32
In6 | int32
In7 | int32
In8 | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In1 | float32
In2 | float32
In3 | float32
In4 | float32
In5 | float32
In6 | float32
In7 | float32
In8 | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In1 | float64
In2 | float64
In3 | float64
In4 | float64
In5 | float64
In6 | float64
In7 | float64
In8 | float64

Outports Data Type
Out | float64