### Block: Asin

Inports
In | Input u

Outports
Out | Result of sin(u)

##### Description:

Arcsine computation of input value.

Calculation:

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
In | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64