### Block: Minimum

Inports
In1 | Input #1
In2 | Input #2

Outports
Out | Minimum of Input #1 and Input #2

##### Description:

Outputs the lesser value of the two input signals.

Calculation:

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In1 | int16
In2 | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In1 | int32
In2 | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In1 | float32
In2 | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In1 | float64
In2 | float64

Outports Data Type
Out | float64