### Block: Atan2

Inports
y |
x |

Outports
Out | Result of atan2(y/x)

##### Description:

Computation of the angle between the inputs x and y.

Calculation:

##### Implementations:

FiP8 | 8 Bit Fixed Point Implementation
FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP8

8 Bit Fixed Point Implementation

Inports Data Type
y | int8
x | int8

Outports Data Type
Out | int8

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
y | int16
x | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
y | int32
x | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
y | float32
x | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
y | float64
x | float64

Outports Data Type
Out | float64