### Block: Saturation

Inports
In | Input

Outports
Out | Limited output

Mask Parameters
max | Upper Limit
min | Lower Limit

##### Description:

Saturation of output to adjustable upper and lower limit.

If the entry for Upper Limit is lower than the entry for Lower Limit then the limits will be swapped internally.

##### Implementations:

FiP16 | 16 Bit Fixed Point Implementation
FiP32 | 32 Bit Fixed Point Implementation
Float32 | 32 Bit Floating Point Implementation
Float64 | 64 Bit Floating Point Implementation

#### Implementation: FiP16

16 Bit Fixed Point Implementation

Inports Data Type
In | int16

Outports Data Type
Out | int16

#### Implementation: FiP32

32 Bit Fixed Point Implementation

Inports Data Type
In | int32

Outports Data Type
Out | int32

#### Implementation: Float32

32 Bit Floating Point Implementation

Inports Data Type
In | float32

Outports Data Type
Out | float32

#### Implementation: Float64

64 Bit Floating Point Implementation

Inports Data Type
In | float64

Outports Data Type
Out | float64